|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **No.** | **Part Number** | **Model** | **Description** | **Unit Qty.** |
|  | **OceanProtect X6000 Backup Storage 1\_Site1** | | |  |
| **1** | **OceanProtect X6000** | | |  |
| **1.1** | **OceanProtect X6000 Main Equipment** | | |  |
| **1.1.1** | **Dual-Controller Unit 1** | | |  |
|  | **SSD&HDD Controller Enclosure** | | |  |
|  | 02355YWH | X6512G2CS25DHAC-OL | OceanProtect X6000(2U,Dual Ctrl,SSD&HDD,SAS,AC\240V HVDC,512GB Cache,4\*(4\*12Gb) SAS,25\*2.5 Inch,SPE53C0225) | 1 |
|  | **Expansion Interface Module** | | |  |
|  | 03050JPF | ODK-SIO4\*32FC-ML | 4 ports SmartIO I/O module(SFP28,32Gb FC) | 2 |
|  | 03050LQE | SMARTIO4\*10E-LL | 4 ports SmartIO I/O module(SFP+,10Gb ETH) | 2 |
|  | **Disk Components** | | |  |
|  | 02356HUP | X9-SSD-SAS-3.84T | 3.84TB SSD SAS Disk Unit(2.5") | 6 |
|  | 02354PCW | OP-NLSAS8T | 8TB 7.2K RPM NL-SAS Disk Unit(3.5") | 35 |
|  | **Disk Enclosure** | | |  |
|  | 02355EYX | DAE62435U4OP | SAS Disk Enclosure(4U,AC\240V HVDC,3.5",Expansion Module,24 Disk Slots,Without Disk Units,DAE62435U4) | 2 |
| **1.2** | **Installation Material** | | |  |
|  | 14130858 | SN2F01FCPC | Patch Cord,DLC/PC,DLC/PC,Multi-mode,3m,A1a.2,2mm,42mm DLC,OM3 bending insensitive | 16 |
|  | 04052252 | HS-SAS-3-02 | High Speed Cable,48G Mini SAS HD Cable,3m,SFF 8644 Plug,28AWG\*4P\*2B(S),SFF 8644 Plug,indoor,SAS 3.0,LSZH,EEPROM | 2 |
| **1.3** | **Software** | | |  |
|  | 88039LSH | LICX6000SW-QY | Dedicated Backup Storage Software Essential License(including 40 TB capacity license) | 1 |
|  | 88039LSM | LICX6000DD1TBS-QY | Dedicated Backup Storage Software Capacity License(41~300TB) | 240 |